Usage: dcm_import [<host> <port> <path> <aetitlescp>]
host       - Destination host.
port       - DICOM port of destination PACSServer.
path       - Path to the folder with DICOM files.
aetitlescp - AE Title of destination server.
Without parameters dcm_import will work in interactive mode.
